| i

| Ambar | Amarillo Neón | Rose Neón | Naranja Neón | Rubí | Topacio |
| Ref: OP-5136 | Ref: OP-5139 | Ref: OP-5143 | Ref: OP-5142 | Ref: OP-5134 | Ref: OP-5131 |
| Turqueza | Agua- marina | Azul Neón | Esme- ralda | Citrón | Circón | Verde Neón |
| Ref: OP-5132 | Ref: OP-5138 | Ref: OP-5140 | Ref: OP-5133 | Ref: OP-5137 | Ref: OP-5135 | Ref: OP-5141 |

| The Opalizzo has been developed highly by Granato as a ornamental solution , directed to create special atmospheres of commercial and advertising use. The Opalizzo is a glossy and translucent surface, not porous, ideal to create welcoming and innovative atmospheres, with a hardness that lets the material be machinable, cutted and polished without difficulty. APPLICATION FIELDS Opalizzo is a fragile material, it is not recommended for applications where it should support weight, neither in areas of high traffic, neither in permanent contact with water nor detergents. . It should not be placed to the bleakness neither with indirect lights.. It is only recommended for ornamental applications, as exhibitors, ornamental panels, advertising modules, etc. PRESENTATION The Opalizzo sheets come in different thickness, dimensions and colors. • 12.7 mm Sheets , 0.74 or 0.88 wide x 3.65 long. • 6 mm Sheets , 0.74 or 0.88 wide x 2.40 long. MANIPULATION AND TRANSPORT Opalizzo is a fragile material that should be manipulated carefully, they are delivered correctlypacked and protected, once received, it's quality must be verified, if it is broken, fissured or overflowed, you must notify immediately to the transport company. to be restored by GRANATO , otherwise GRANATO won't assume any type of responsibility for damage caused on the sheets. STORAGE It is recommended to store the sheets, without the packing protection, in horizontal way, never vertical, placing cardboards between the sheets to avoid possible scratches. |

Granato, the versatile and resistant solid surface. Easy to work as wood. |

| INSTALATION The Opalizzo is a not structured material that can present bulges or deformation with temperature changes, it is recommended during its installation the structuring or support with a mark or metallic plate always in its four sides. MAINTENANCE The Opalizzo is easy and quick to clean, it is recommended to clean it with a soft cloth and glass cleaner, so that it conserves its characteristics, when the surface is greased , clean it with isopropilic alcohol TECHNICAL ASSISTANCE Granato has a highly qualified technical service that supports the best use and perfomance of our products. |

TECHNICAL SPECIFICATIONS
Characteristic | Value | Checkup method
Specific gravity, 25oC | 1.14 | ASTMD D-792
Hardness Barcol (model GYZJ 934-1) | 35 | ASTMD D-2583
Tension Resistance, MPa | 66 | ASTMD D-638
Tensil Module, GPa | 2.96 | ASTMD D-638
Elongation in the rupture, % | 4.8 | ASTMD D-638
Flexion Resistance, MPa | 105 | ASTMD D-790
Flexion Module, MPa | 2700 | ASTMD D-790
Water Absorption in 24 hours, mg | 17.9 | ASTMD D-570
Note: 1MPa = 1MN/m2 = 1N/mm2 = 145,04 psi 1 GPa = 1000 MPa

| The information and recommendations described here, are entirely reliable. Offered suggestions for uses or applications are only the GRANATO'S opinion . The consumers will make their own tests to determine the behavior of this product in their specific objectives. GRANATO only guarantees the product's standard technical specifications. |