| i

| Oriental Geige | Cafetto | Limone | Azabache | Carbonio | Azahar Blanco |
| Ref: S1-1261 | Ref: S1-1361 | Ref: S1-1761 | Ref: S1-2061 | Ref: S1-2071 | Ref: S3-1121 |
| Miele | Acacia | Granate | Gris Tempo | Cristallo | Satino Beige |
| Ref: S3-1221 | Ref: S3-1721 | Ref: S3-1821 | Ref: S3-1921 | Ref: S4-1101 | Ref: S4-1211 |

| Platino | Earth | Green Mount | Aurus | Artstone | Eclectic |
| Ref: S4-1911 | Ref: S3-1311 | Ref: S3-1711 | Ref: S3-1951 | Ref: S3-1411 | Ref: S3-1511 |
| Sea Jewel | Star Night | Mith Grey | Ethnic | Native Gen | Sahara Sand | Greenish |
| Ref: S3-1611 | Ref: S3-2011 | Ref: S3-1941 | Ref: S3-1211 | Ref: S3-1811 | Ref: S3-1931 | Ref: S3-1731 |

| Granato is an ideal solution for surfaces and veneer handling in your works and projects, its versatility, easy handling and maintenance, make this product to be adapted perfectly to the kitchen tables necessities in general Granato is the result of a mixture of non porous synthetic and homogeneous materials that when united and heat postcured acquires special characteristic of hardness, resistance to impacts, heat, stripes, ultraviolet rays, chemicals and acids among others, The result is a material that seems stone and its worked as wood, with the same tools with which this one is transformed. The grains that confer the appearance to this product, go through the whole surface in a homogeneous way, what allows to unite sheet with sheet in all the directions, with totally imperceptible ties. APPLICATION FIELDS Granato is an ideal material for veneers and kitchen tables, bathrooms, laboratory, attention counters, tables, desk covers, open office panels and a thousand more utilities. PRESENTATION The Granato sheets come in different thickness, dimensions and colors. • 12.7 mm Sheets , 0.76 or 0.90 wide x 3.68 long (21 Kg/m2). • 6 mm Sheets , 0.76 or 0.90 wide x 2.40 long (7 Kg/m2). FINISHES Mate, Shine and Brilliant. From the factory the product has a mate finishes. Another finishes type should be specified to the transformer. The brilliat finishes requires bigger care and maintenance. We Recomend a dull and shine finishes for kitchen tables and high use food counters. The color between sheet and sheet can vary slightly. T RANSPORT AND MANIPULATION Granato sheets must be manipulated carefully, they are delivered correctly packed and protected, once received, it's quality must be verified, if it is broken, fissured or overflowed, you must notify immediately to the transport company. STORAGE It is recommended to store the sheets, without the packing protection, in horizontal way, never vertical, placing cardboards between the sheets to avoid possible scratches. MAINTENANCE Granato can last unalterable in the time, carrying out periodically a quite simple maintenance , similar to polishing a fine wooden piece of furniture or a silver piece. See Maintenance Manual . TRANSFORMING AND INSTALLATION Granato puts at your disposal a highly qualified technical department that will give you instructions on the correct way to manipulate, transform and install the surfaces. PHYSIC - CHEMICAL PROPERTIES The most common characteristics under the ANSI norms (American National Standards lnstitute),ASTM (American Society for Testing and Materials) and NEMA, that rules for materials like the solid surface are:
Density The density refers to the mass of the material by volume unit , measure in gr/cm3. For Granato it is 1,72 g/cm3, what is equal to 24,87 kg/M2.
Hardness The hardness is measured in the Barcol scale, internationally accepted for this class of materials, Granato presents a hardness that oscillates between 55 and 58 Barcol, being this, one of the characteristics that makes it machinable.
Water absortion It refers to the weight gained by the material when submerged for a specific time in water . Granato is a homogeneous material, porosity lacking, its water absorption degree is 0,02% in weight when it is submerged during 24 hours, thus leading to a high humidity resistance . This property makes Granato an inorganic and aseptic material.
Flame retardant Granato is designed with fireproof preservatives that makes of this an auto extinguishable and slow combustion product. A lit cigarette can be left until wasting away, only leaving a superficial yellow color that can be retired easily as explained in the repair manual. Granato can be dived in boiling water up to 65oC during 100 hours without showing bladders, cracks, peelings or cracking in its surface.
Impact test on spherical fall Granato doesn't present effect to the impact test on spherical fall (1/2 pound, of solid plumb), from 2,44M height, according to norm ANZI Z.125.
Resistance to microorganisms and bacterias Granato is an inert and not porous surface that doesn't allow bacteria growth, thats why it is recommended for restaurants services , surgery rooms,laboratories, etc, doesn't house microorganisms nucleus or polluting substances.
C hemic al resistance Granato has been subjected to different tests, showing a good perfomance to the contact with multiple chemical substances as naphtha, ethylic alcohol, amilo acetate, ammonia (watery solution at 10%), citric acid (watery solution at 10%), urea at 6%, peroxide of hydrogen (solution watery at 3%), sodium hypochlorite , toluene, ethyl acetate. Also, it can't be stained with hair dye, polish, stamp tints and indelible marker. If a bleaching or opacity appears in the surface, GranatoŽ is recoverable easily as explained in the recovery manual. To know the chemical resistance to a specific substance, it is suggested to consult our advisers.
TECHNICAL SPECIFICATIONS |

Properties | Granato | Checkup method
Specific gravity | 1.72 | ASTMD D-792
Hardness (Barcol) | 55-58 | ASTMD D-2583
Tension resistance (PSI) | 4.300 | ASTMD D-638
Tension module (x106) | 1.28 | ASTMD D-638
Elongation | 0.5 | ASTMD D-638
Flexion resistance (PSI) | 5.930 | ASTMD D-790
Abrasion resistance. In grams weight loss at 500 cycles | 0.14 | ASTMD D-4060
Water absorption % weight/24 Hrs. | 0.02 | ASTMD D-570
Impact IZOD, foot pound/inch | 0.55 | ASTMD D-256
Impact by spherical fall (sphere 1/2 pound) | 2.44 mt. (without effect) | ANSI Z. 125
Heat resistance | pass | NEMA D-2863
Water boiling resistance | pass | NEMA LD 3-85
Spott resistance | pass | ANSI Z-124
Chemical resistance | pass | ANSI Z-124

Multiple applications: Veneers, signaling, interior facades, kitchen sinks, vanity bowls,architectural details. |