|  | i

| Practical solution to burns | Cuts or rayons | In few words
| Granato is an easy recovery surface. To repair smaller damages, we give some recommendations that you can put easily into practice. In the event of bigger accidents as fissures or splinters, they can be repaired calling the manufacturer or directly in our offices, we will put in your hands all the available technology to solve any problem.

| PRACTICAL SOLUTION TO BURNS The lit cigarettes placed on Granato can cause small burns if they are left a lot of time there. If this happens, there are several possible solutions. First , rub the burn with a Scotch Brite industrial cloth No. 7448 , you can get it with a 3M distributor , with abrasive kitchen soap, Axión,Tras, etc.) and some water. If it is not enough pass on the surface sandpaper grain 320 with water and pass the Scotch Brite cloth again as seen previously. Keep in mind that if the Granato's surface has a satin finishes, it is necessary to shine the sanded area . For it, apply Pintuco's white stain cream for cars ref: 20025 with a cotton cloth and if the finish is brilliant, subsequently apply liquid car wax for cars neuter color or a kindred color to the surface (C.R.C., Simoniz, etc.).
| C UTS O R RAYONS In case the surface suffers some cut or rayon, this is repaired easily when rubbing on it sandpaper for water grain 120 or 220, 320 considering the depth of the rayon. If it is deep, use sandpaper 120 and water , rub later sandpaper 220 and Scotch Brite as it was explained in the previous point (PRACTICAL SOLUTION TO BURNS). If the scratch is not very deep, start the process with sandpaper # 220 and finish with 320. Don't forget to shine if it is necessary.
IN FEW WORDS Granato is a surface of easy maintenance and repair, of simple daily cares, that guarantee its good conditions the whole time. Follow the previously suggested instructions for maintenance and small accidents solution. It will always maintain the Granato in perfect conditions. Please read the Services section.